





TC\_M firmware update instructions

1. Connect the machine to the PC via USB cable.
2. Double click to run the tool “CBW\_Upgrade\_V2.0.exe”.   
   
3. Click the button “Browse” to select the flash file for the firmware.   
     
   
4. Click the button “Upgrade”. It prompts message “Current Version is xx.xx, Continue?”.  
   
5. Click the button “OK”. The progress bar start to move.   
   
6. When the progress bar moves to 100%, it prompts “Finish OK!”   
   
7. Click the button “OK” to finish the firmware upgrading process.
8. The machine should restart itself. If the machine doesn’t restart automatically, please restart the machine manually(power off and power on).
9. That’s all.